About heart beat

1. our socket packet design:

u\_int8 1024byte u\_int32

Packet content

Packet length

Packet type(0/1)

packet type 0: heart beat;

packet type 1: normal socket message content;

packet type 2: user information(account & password and so on);

packet content: packet real content;

packet length: packet length, including self;